<?xml version="1.0" encoding="UTF-8"?>
<WindTurbineGenerator FormatVersion="1.01" Description="Vestas V60-850 kW" ManufacturerName="Vestas Wind Systems A/S" ReferenceURI="www.vestas.com" RotorDiameter="60"><Comments>Address: Alsvej 21, 8940 Randers, Denmark|Phone: +45 97 30 00 00|Fax: +45 97 30 00 01|E-mail: vestas@vestas.com</Comments><SuggestedHeights><Height>60.0</Height></SuggestedHeights><PerformanceTable AirDensity="1.225" MaximumNoiseLevel="0.0" BladePitchAngle="-99999.0" DataStatus="Unknown" DataSource="Document no.: 1000001 V03" ReleaseDate="2010-02-24" ReferenceURI="None" StationaryThrustCoEfficient="0.081"><StartStopStrategy LowSpeedCutOut="3.0" LowSpeedCutIn="3.0" HighSpeedCutIn="20.0" HighSpeedCutOut="20.0"/><Comments></Comments><DataTable><DataPoint WindSpeed="3.0" PowerOutput="10000.0" ThrustCoEfficient="0.0"/><DataPoint WindSpeed="4.0" PowerOutput="33000.0" ThrustCoEfficient="0.872"/><DataPoint WindSpeed="5.0" PowerOutput="86000.0" ThrustCoEfficient="0.833"/><DataPoint WindSpeed="6.0" PowerOutput="160000.0" ThrustCoEfficient="0.832"/><DataPoint WindSpeed="7.0" PowerOutput="262000.0" ThrustCoEfficient="0.832"/><DataPoint WindSpeed="8.0" PowerOutput="398000.0" ThrustCoEfficient="0.832"/><DataPoint WindSpeed="9.0" PowerOutput="568000.0" ThrustCoEfficient="0.825"/><DataPoint WindSpeed="10.0" PowerOutput="732000.0" ThrustCoEfficient="0.778"/><DataPoint WindSpeed="11.0" PowerOutput="836000.0" ThrustCoEfficient="0.539"/><DataPoint WindSpeed="12.0" PowerOutput="847000.0" ThrustCoEfficient="0.387"/><DataPoint WindSpeed="13.0" PowerOutput="850000.0" ThrustCoEfficient="0.295"/><DataPoint WindSpeed="14.0" PowerOutput="850000.0" ThrustCoEfficient="0.232"/><DataPoint WindSpeed="15.0" PowerOutput="850000.0" ThrustCoEfficient="0.187"/><DataPoint WindSpeed="16.0" PowerOutput="850000.0" ThrustCoEfficient="0.154"/><DataPoint WindSpeed="17.0" PowerOutput="850000.0" ThrustCoEfficient="0.129"/><DataPoint WindSpeed="18.0" PowerOutput="850000.0" ThrustCoEfficient="0.109"/><DataPoint WindSpeed="19.0" PowerOutput="850000.0" ThrustCoEfficient="0.093"/><DataPoint WindSpeed="20.0" PowerOutput="850000.0" ThrustCoEfficient="0.081"/></DataTable></PerformanceTable><ContextInformation><CertificateChecksum></CertificateChecksum></ContextInformation></WindTurbineGenerator>
